Jeep has been lifted and modified for rock crawling with the following-
Front and rear ARB lockers
SS-214 3.5” lift
Poison Spyder: front & rear bumpers, tire carrier, rock sliders, fenders, body armor and beadlocks
Front and rear anti-rock sway bars
Dynatrac ProRock 44/60 axles
King Air bump stops
Metalcloak adjustable control arms
Reid racing knuckles with 1 ton high steering
Warn winch
Hydraulic steering assist
Skid plates

sPod switch panel

New battery
Tires are 37” but need to be replaced. Small leak in oil pan, bolts holding tire carrier need replaced. No other known issues.